SPANISH

**Reference Project Name: Punto Horizonte**

**CATEGORY: FINISHES, CERAMIC TILES,**

Project Overview:

Se tenía el requerimiento de generar los acabados a la Torre 2 de punto Horizonte, tanto en interiores como en exteriores, de igual manera se tenía que escoger entre un adhesivo y boquilla para poder aplicar las piezas de mármol 60\*40 que lleva el edificio.

* **Explain the Mapei solution:**
* Después de generar pruebas de aplicación y de competir contra Cemix en los acabados 8estuco, BaseCoat) y USG en paneles ligeros (Readymix) el cliente se decanta por nuestra solución

**APLICACIÓN DE ACABADOS EXTERIORES**

1.- MORTEX REPELLO para muros a plomo.

2.- MORTEX PLUS como acabado final en muros.

3.- MORTEX BASECOAT para aplicación en placas de fibrocemento y yeso.

4.- READY MIX para calafateo de placas de yeso en interiores.

**APLICACIÓN DE PISO INTERIOR Y AREAS PÚBLICAS**

1.- KERABOND PORCELANICO para la aplicación de losetas.

2.- KERACOLOR FF como boquilla para terminado.

**Project Background**

PUNTO HORIZONTE es un conjunto de torres de tipo residencial ubicadas en el exclusivo fraccionamiento Lomas de Angelopolis, ubicado en la ciudad de Puebla, cuenta con 20 niveles y es considerado uno de los edificios de mayor lujo en la zona.

**Project information**

Period of construction: 2019-2021

Year of MAPEI involvement: 2020-2021

MAPEI Coordinator: ARTURO LUNA SANCHEZ

Project Owner: GRUPO PROYECTA.

MAPEI Distributors: EGMC CONSTRUCTOR SA DE CV

Architect: OMAR GARCIA

General Contractor: EGMC CONSTRUCTOR SA DE CV

Surface preparation contractor: 15,400 M2

Tile and stone installers: EGMC CONSTRUCCION

Project manager: ING. CARLOS GARCIA

Photographer: ARTURO LUNA

Project size: 80,000.00 M2

**MAPEI products used**

* *MORTEX REPELLO*
* *MORTEX PLUS*
* *KERABOND PORCELANICO*
* *KERACOLOR FF*
* *READIMIX*
* *MORTEX BASECOAT*

**MAPEI products at work on the jobsite:**

* Se aplica MORTEX REPELLO PARA DEJAR MUROS A PLOMO
* Se aplica MORTEX PLUS PARA ACABADO EN EXTERIORES
* Se aplica KERABOND PORCELANICO PARA APLICACIÓN EN PISO.
* Aplicación de MORTEX BASECOAT PARA APLICACIÓN EN FIBROCEMENTO
* Aplicación de KERACOLOR FF COMO BOQUILLA

**ENGLISH:**

**Reference Project Name: Horizon Point Residential**

**CATEGORY: FINISHES, CERAMIC TILES,**

**Project Overview:**

There was a requirement to generate the finishes to the Horizon Point Tower 2, both indoors and outdoors. In accordance with there was the requirement to propose an adhesive or a grout to apply in the joints of the 60 \* 40 marble pieces.

• **Explain the Mapei solution:**

• After carrying out the corresponding tests, competing against Cemix in the stucco finishes as Mortex BaseCoat, and USG in the light panels finishes like Ready Mix, the client chooses the Mapei solution

**APPLICATION OF EXTERIOR FINISHES**

1. - MORTEX REPELLO for plumb walls.

2. - MORTEX PLUS as a final finish on walls.

3. - MORTEX BASECOAT finishes fiber cement and plasterboards.

4. - READYMIX for interior plasterboard finishing.

**INTERIOR FLOOR APPLICATION AND PUBLIC AREAS**

1. - KERABOND PORCELANICO ceramic tile adhesive.

2. - KERACOLOR FF grout for tiles

**Project Background**

PUNTO HORIZONTE is a set of residential towers located in the exclusive Lomas de Angelopolis subdivision, in Puebla, it has 20 levels and is considered one of the most luxurious buildings in the area.

**Project information**

Period of construction: 2019-2021

Year of MAPEI involvement: 2020-2021

MAPEI Coordinator: ARTURO LUNA SANCHEZ

Project Owner: GRUPO PROYECTA.

MAPEI Distributors: EGMC CONSTRUCTOR SA DE CV

Architect: OMAR GARCIA

General Contractor: EGMC CONSTRUCTOR SA DE CV

Surface preparation contractor: 15,400 m2

Tile and stone installers: EGMC CONSTRUCCION

Project manager: ING. CARLOS GARCIA

Photographer: ARTURO LUNA

Project size: 80,000.00 m2

**MAPEI products used**

1. - MORTEX REPELLO for plumb walls.

2. - MORTEX PLUS as a final finish on walls.

3. - MORTEX BASECOAT finishes fiber cement and plasterboards.

4. - READYMIX for interior plasterboard finishing.

INTERIOR FLOOR APPLICATION AND PUBLIC AREAS

1. - KERABOND PORCELANICO ceramic tile adhesive.

2. - KERACOLOR FF grout for tiles